MOV EAX,[EBP-pv_CONDITION1@IFSTATEMENT]
PUSH EAX
PUSH DWORD [EBP-pv_CONDITION2@IFSTATEMENT]
CALL [EDI+xf_STRCMP]
TEST EAX,EAX
JNZ if12
LEA EAX,[ESI+else12]
JMP EAX
if12:
MOV DWORD [EBP-lv_IFSTATEMENT@IFSTATEMENT],1
LEA EAX,[ESI+endif12]
JMP EAX
else12:
MOV DWORD [EBP-lv_IFSTATEMENT@IFSTATEMENT],0
endif12:
